
The universal X-Ray film fixer system for automatic processing machines.
· Long level of sulphur dioxide emission from working solutions
· Very clean working 
· Optimised replenishment rates 
· Suitable for the processing of all currently available Medical and Industrial Radiographic and Imaging films 
· Readily introduced by replenishment to existing solutions 
· For use in all automatic processing machines at all time cycles
· Packs available for all chemical mixers
· Full office based and field based technical support
Processing of all film materials compatible with the HiS X-RAY FIXER system.

Fixer temperature
The temperature of the fixer bath should be set the same as for the developer bath.

Replenishment Rates

	General Departments
	550 – 730 ml/m²
	(70 – 90 ml/350 x 350 mm film)

	Specialist Departments
	480 – 820 ml/m²
	(60 – 100 ml/350 x 350 mm film)


The above recommendations are based on the requirements of a general hospital department and when specialised techniques are employed the fixer injection rates should be modified by plus or minus 10 – 15%.

Preparation of Solutions
Full details concerning the preparation of HiS X‑RAY FIXER solutions are provided either on the pack labels, or with the concentrates, and these should be followed carefully.  NB:  Any information concerning chemical preparation, marked on the processing machine, or printed in the machine handbook, should be disregarded if it conflicts with the recommendations printed on the HiS X‑RAY FIXER packs or in this leaflet.
NOTE:  Extreme care should be taken to avoid cross-contamination of the developer solutions with fixer, since even small volumes of fixer in the developer will cause large processing variations.
Before a tank is refilled, it should be completely drained, thoroughly cleaned with PROCESSOR SYSTEMS CLEANER, and flushed out with water. 

Preparation of Initial Tank Solutions
The same solution as for replenishment is used for the initial filling of the machine fixer tank.
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Storage
Concentrates:  All of the HiS X-RAY FIXER processing system concentrates have a normal storage life of at least 12 months, when held in full, tightly capped containers under steady temperature conditions in the range 13 – 18 ºC.  However, storage temperatures below 5 ºC should be avoided as some crystallisation may occur.
Working Strength Solutions:  The vat life of fixer replenisher is 3 – 6 months under temperate (13 – 18 ºC) conditions.  At higher ambient temperatures this may be reduced by at least 50%.
Safe Use of Processing Chemicals
All chemicals should be kept out of reach of children. 
The precautionary information, printed on the pack labels, should always be read before the chemicals are used.
Protective clothing, including gloves and face/eye protection should always be worn when handling chemicals.
In the event of accidental contact with solutions, or solid chemicals, the skin should be rinsed with running water, while the eyes should be rinsed for at least 15 minutes and MEDICAL ADVICE sought.

















Supplies
	9X23012
	HiS X-RAY FIXER 
Compak to make 2 x 20 litre

	9X230120A
	HiS X-RAY FIXER 
Compak to make 1 x  20 litre 

	9X23031A
	HiS X-RAY FIXER 
Ready to use 20 litre Bag-in-Box

	9X23013
	HiS X-RAY MANUAL FIXER 
6 x 1 litres to make 30 litres

	9X2300F
	HiS X-RAY FIXER SYSTEMS CLEANER
To make 2 x 20 litres

	
	

	
	














Manufactured in South Africa for:
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58 Stanhope Road, Wychwood, Germiston. P.O. Box 751954, Gardenview, 2047
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